**GREEN BUILDING STORE SPECIFICATION**

Environmental Construction Products Ltd

T/A Green Building Store

Heath House Mill

Golcar

Huddersfield

HD7 4JW

Tel: 01484 463336 (High Performance Windows Department) 461705 (Main Switchboard)

Email: info@greenbuildingstore.co.uk

Web: [www.greenbuildingstore.co.uk](http://www.greenbuildingstore.co.uk)

Contact: Paul Cowley

**PRODUCT REFERENCE**

GBS PERFORMANCE triple glazed sliding doorset

**GENERAL SPECIFICATION**

**AIRTIGHTNESS**

All doorsets shall have integral draught seal(s) all round.

All doorsets shall have proof of performance by independent third party certification to BS EN 12207:2016 Class 4 600 Pa

**WEATHERPROOFING**

All doorsets shall have proof of performance by independent third party certification to exposure category in accordance with BS 6375-1:2015 not less than 1200

**TIMBER SOURCING**

All doorsets shall carry Forest Stewardship Council Chain of Custody with FSC 100% certification.

**SAFETY GLAZING**

All glass shall be of the required specification to meet safety requirements in accordance with Building Regulations Approved Document K.

All glass shall be suitable to meet anticipated wind loads according to BS6262-3:2005

All glass specified as a barrier or balustrade to protect from falls shall be in accordance with the requirements of Building Regulations Approved Document K and BS6180:2011

# All glazing shall be with triple glazed, hermetically sealed units manufactured to BS EN 1279-5:2005+A2:2010 with soft coat low emissivity coatings (ε ≤ 0.05) at positions 2 & 5 as measured from the exterior, Argon fill 90% and warm edge spacers (Ψ ≤ 0.040). U value of standard glazing shall be ≤ 0.60 W/m2K and g value ≥ 50%.

**SECURITY**

All doorsets shall be high security accredited by Secured by Design *(required for Part Q compliance in England)*

**THIRD PARTY CERTIFICATION**

Doorsets shall be manufactured under independent UKAS approved third party certification.

**INSTALLATION**

All doorsets to be installed by FENSA registered installers.

All doorsets shall be mechanically fixed according to the manufacturer’s specification, plumb and square.

All doorsets shall be sealed to the external substrate according to the manufacturer’s specification or according to contractor’s choice, to be approved.

All doorsets shall be installed with proprietary airtightness tapes and mastics to achieve high levels of installation airtightness.

After installation all doorsets shall be checked for operation, and if necessary mechanisms shall be adjusted and lubricated prior to hand over to the client.

**COMPOSITE FRAMES**

All composite frames shall be assembled according to manufacturer’s specification and shall ensure that joints are weather and air tight.

**PROTECTION ON SITE**

All doorsets shall be stored on site according to manufacturer’s specification, and generally off the ground, fully protected from wind and rain under cover and adequately ventilated.

After installation site ambient moisture levels shall be maintained such that moisture content within frames at no times rises above 17%.

All doorsets shall be protected to avoid site damage at all times. Where plaster or other contaminants are deposited on frames they shall be removed immediately to avoid risk of site damage.

**PRODUCT STANDARD PROPERTIES**

Frame and sash depth

 78 mm

Maximum sizes

 Single opening door and fixed light 5500mm x 2400mm

Finish

 Full factory treatment and finish from Remmers Baustofftechnik

Hardware

Siegenia Aubi Portal HS300 lift and slide

GBS proprietary high security supplementary lock

Pair of half Euro cylinders, generic 1\*

Sills

Siegenia Aubi Ecopass composite GRP and aluminium

Glazing spacers

 Swisspacer warm edge

Glazing

 44 mm triple glazed toughened units, 2 x soft coat low-E, Argon fill 90%

 Standard configuration 4Tgh.E-16A-4Tgh-16A-E.Tgh4 (E – low E coating; A – Argon 90%)

 Standard Ug 0.58 W/m2K

Thermal insulation values

 Ud = 1.0 W/m2K (Redwood) \*

 Ud = 1.1 W/m2K (Oak) \*

\**(2000mm x 2180mm as BS EN 14351:2001 +A1:2010)*

**PRODUCT PROPERTIES TO BE SPECIFIED**

Sash & frame material

 [ FSC 100% fair-faced engineered Oak ]

 [ FSC 100% finger-jointed engineered Redwood ]

Interior finish

 [ Clear ]

 [ Painted, RAL \_\_ ]

 [ Woodstain Afromosia ]

 [ Woodstain Afzelia ]

 [ Woodstain Oak ]

 [ Woodstain Pine ]

 [ As exterior ]

Exterior finish

 [ Painted, RAL \_\_ ]

 [ Woodstain Afromosia ]

 [ Woodstain Afzelia ]

 [ Woodstain Oak ]

 [ Woodstain Pine ]

Glazing

 [ Toughened ]

 [ Toughened + Laminated (inner) (middle) (outer) ]

 [ Toughened + Obscure, pattern \_\_\_ ]

 [ Toughened Self cleaning ]

 [ Toughened Solar control, g = \_\_\_ ]

 [ Toughened Acoustic ]

Glazing spacer

 [ Grey ]

 [ Black ]

 [ White ]

Gasket

 [ Grey ]

Handle colour

 [ Matt silver ]

 [ Gold ]

 [ White ]

 [ Brown ]

Cylinder type

[ Keyed ]

 [ Suited keyed alike ]

[ Thumb turn ]

Security

 [ Standard ]

 [ Secure by Design ]

**CERTIFIED PERFORMANCE**

Performance BS6375-1,2,3 (test certificates available)

 BS EN 12207 Air permeability Class 4 600 Pa

 BS EN 12208 Water tightness Class 3A 100 Pa

 BS EN 12210 Wind loads Class C4 1600 Pa

 BS 6375-1:2009 Exposure category 1200

 BS 6375-2:2009 Pass

 PAS24:2012 Pass

**CERTIFICATION**

* Secured by Design
	+ Standard: Licence
	+ Details: Licensed products – windows, single doors, double doors, sliding doors
* CEN Solutions
	+ Standard: CMS 3165 WDG Gold
	+ Details: third party certification
* Forest Stewardship Council
	+ Standard/Certificate: SA-CoC-001435
	+ Details: FSC 100% and FSC Mix products in European Redwood and Oak
* CE Marking
	+ Declaration of Performance <http://www.greenbuildingstore.co.uk/about/ce-mark/>